# FRONT APRON TO COWL SIDE MEMBER > ASSEMBLY REPLACEMENT

1. With the front fender front apron and cowl top side panel removed.

REMOVAL

Symbol meaning
| Remove Weld Points
| Remove Weld Points
| Remove Weld Points

REMOVAL POINT

1. After removing the front apron to cowl side lower front member, remove the front apron to cowl side member.

INSTALLATION

Symbol meaning
| Plug Weld
| Plug Weld
| Plug Weld

INSTALLATION POINT

1. Inspect the fitting of the related parts around the new parts before welding. This affects the appearance of the finish.
2. Temporarily install the new parts and measure each part of the new parts in accordance with the body dimension diagram. (See the body dimension diagram)
3. After welding the front apron to cowl side member to the vehicle side, install the front apron to cowl side lower front member.
4. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.