# REAR FLOOR SIDE MEMBER > ASSEMBLY REPLACEMENT

1. With the body lower back panel removed.

REMOVAL

Symbol meaning
| Remove Weld Points
| Remove Weld Points

INSTALLATION

Symbol meaning
| Plug Weld
| Plug Weld
| Assembly Mark

INSTALLATION POINT

1. For positioning of the new parts, align the installation standard holes of the rear floor side rear member and the member.
2. Temporarily install the new parts and measure each part of the new parts in accordance with the body dimension diagram. (See the body dimension diagram)
3. After welding, apply undercoating to the corresponding parts. (See the paint / coating)
4. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.