# FRONT SUSPENSION CROSSMEMBER > TWO-DIMENSIONAL DISTANCE

HINT:

1. Length measurements are indicated at the points where the arrows extending from the zero point intersect the lines that extend towards the outside of the illustration from each point.
2. Point C, c on the vehicle are asymmetrical.
3. In cases in which only one dimension is given, left and right are symmetrical.

1. For symbols, capital letters indicate right side of vehicle, small letters indicate left side of vehicle (seen from rear).

Measuring Point Name
Symbol | Name | Hole Diameter mm (in.)
A, a | Front Suspension Lower Arm Installation Hole | φ17.5 (0.69)
B, b | Front Suspension Crossmember Installation Hole (Lower) | φ22 (0.87)
C, c | Front Suspension Crossmember Standard Hole | φ12 (0.47)
D, d | Steering Gear Box Installation Hole | φ17 (0.67)
E, e | Front Suspension Lower Arm Installation Hole | 21X18.5 (0.83X0.73)
F, f | Front Suspension Crossmember Installation Hole | φ22 (0.87)