# RADIATOR SUPPORT > ASSEMBLY REPLACEMENT

REMOVAL

Symbol meaning
| Remove Weld Points

REMOVAL POINT

1. *1: Bolts.

INSTALLATION

Symbol meaning
| Plug Weld

INSTALLATION POINT

1. Inspect the fitting of the related parts around the new parts before welding. This affects the appearance of the finish.
2. Temporarily install the new parts and measure each part of the new parts in accordance with the body dimension diagram. (See the body dimension diagram)
3. *1: Bolts.
4. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.
5. Measure the dimensions before installing the headlights.

Reference Value
Area | Measurement | Area | Measurement
*a | 1382 mm (54.41 in.) | *b | 918 mm (36.14 in.)
*c | 981 mm (38.62 in.) | *d | 915 mm (36.02 in.)
*e | 900 mm (35.43 in.) | *f | 130.2 mm (5.13 in.)