# FRONT FENDER FRONT APRON > ASSEMBLY REPLACEMENT

1. With the radiator upper side support removed.

REMOVAL

Symbol meaning
| Remove Weld Points
| Remove Weld Points
| Remove Weld Points

INSTALLATION

Symbol meaning
| Spot Weld
| Plug Weld
| Plug Weld
| Plug Weld

INSTALLATION POINT

1. Inspect the fitting of the related parts around the new parts before welding. This affects the appearance of the finish.
2. Temporarily install the new parts and measure each part of the new parts in accordance with the body dimension diagram. (See the body dimension diagram)
3. When welding *1, make a hole on a new part for plug welding and weld the panel with the panel behind completely.
4. After welding, apply body sealer and undercoating to the corresponding parts. (See the paint / coating)
5. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.