# UNDER BODY REFERENCE VALUES > THREE-DIMENSIONAL DISTANCE

HINT:

1. Measure points with the engine under cover NO.1 and front floor cover removed.
2. Point A, a and B, b on the vehicle are asymmetrical.
3. In cases in which only one dimension is given, left and right are symmetrical.

1. For symbols, capital letters indicate right side of vehicle, small letters indicate left side of vehicle (seen from rear).

Measuring Point Name
Symbol | Name | Hole Diameter mm (in.)
A, a | Side Rail Reinforcement Rear Installation Bolt | M12 (0.47)
B, b | Side Rail Reinforcement Rear Installation Bolt | M12 (0.47)
C, c | Front Suspension Member Installation Bolt | M14 (0.55)
D, d | Front Suspension Member Installation Bolt | M14 (0.55)
E, e | Front Side Member Standard Hole | φ18 (0.71)