# NAME PLATE > ATTACHMENT POSITION

1. Heat the double-sided tape remaining on the body with an infrared lamp or equivalent.

   HINT:
     Heat the tape to 40 to 60°C for approximately 1 to 2 minutes.
2. Wipe off the remaining double-sided tape using a clean cloth or equivalent.

   NOTICE:
     If a name plate is installed without thoroughly removing the remaining double-sided tape from the body, the name plate will not adhere properly. Make sure to thoroughly wipe off the double-sided tape.
3. After cleaning the installation area of the body with degreasing agent, attach the name plate to the position shown in the illustration.

   HINT:
     The working environment should be 20°C when installing the name plate. If the working environment is below 20°C, heat the installation area of the body to 20 to 30°C and then install the name plate.

Text in Illustration
*1 | NO. 1 BACK DOOR NAME PLATE | *2 | NO. 2 BACK DOOR NAME PLATE
*3 | BODY SIDE NAME PLATE | *4 | NO. 2 FRONT FENDER NAME PLATE
*5 | NO. 1 FRONT FENDER NAME PLATE | *6 | Profile of Back Fender Panel
*7 | Profile of Back Fender Panel | *8 | Profile of Front Fender Panel
*9 | Profile of Front Fender Panel | *10 | Profile of Rear Door Panel

Reference Value
Area | Measurement | Area | Measurement
*a | 30.7 mm (1.21 in.) | *b | 66.9 mm (2.63 in.)
*c | 131.1 mm (5.16 in.) | *d | 29.7 mm (1.17 in.)
*e | 65.0 mm (2.56 in.) | *f | 130.6 mm (5.14 in.)
*g | 34.2 mm (1.35 in.) | *h | 47.7 mm (1.88 in.)
*i | 52.6 mm (2.07 in.) | *j | 47.2 mm (1.86 in.)
*k | 112.1 mm (4.41 in.) | *l | 55.8 mm (2.20 in.)
*m | 54 mm (2.13 in.) | *n | 47.2 mm (1.86 in.)
*o | 112.1 mm (4.41 in.) | *p | 55.8 mm (2.20 in.)
*q | 54 mm (2.13 in.) | - | -