# ROOF PANEL (w/o Sliding Roof) > ASSEMBLY REPLACEMENT

REMOVAL

Symbol meaning
| Remove Weld Points
| Remove Weld Points

INSTALLATION

Symbol meaning
| Spot Weld
| Plug Weld
| Plug Weld
| Body Sealer

INSTALLATION POINT

1. Inspect the fitting of the related parts around the new parts before welding. This affects the appearance of the finish.
2. Temporarily install the new parts and measure each part of the new parts in accordance with the body dimension diagram. (See the body dimension diagram)
3. Before temporarily installing the new parts, apply body sealer to the windshield header panel, roof panel reinforcement and back door opening frame.

   HINT:
     Apply just enough body sealer for the new parts to make contact.
4. After the roof panel reinforcement is welded to the new parts, install the roof panel to the vehicle side.
5. After welding, apply the foamed sealing material to the corresponding parts. (See the paint / coating)
6. After welding, apply body sealer to the corresponding parts. (See the paint / coating)
7. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.