# REAR DOOR > THREE-DIMENSIONAL DISTANCE

HINT:

1. In cases in which only one dimension is given, left and right are symmetrical.

1. For symbols, capital letters indicate right side of vehicle, small letters indicate left side of vehicle (seen from rear).

Measuring Point Name
Symbol | Name | Hole Diameter mm (in.)
A, a | Roof Side Rail Assembly Mark | -
B, b | Rear Door Hinge Installation Nut | M8 (0.31)
C, c | Rear Door Hinge Installation Nut | M8 (0.31)
D, d | Center Body Pillar Assembly Mark | -
E, e | Center Body Pillar Assembly Mark | -
F, f | Rocker Panel Assembly Mark | -
G, g | Roof Side Rail Assembly Mark | -
H, h | Quarter Panel Assembly Mark | -
J, j | Quarter Panel Assembly Mark | -
K, k | Rear Door Lock Striker Installation Nut | M8 (0.31)