# REAR FLOOR LOWER FRONT CROSSMEMBER > ASSEMBLY REPLACEMENT

1. With the rear floor pan removed.

REMOVAL

Symbol meaning
| Remove Weld Points
| Remove Weld Points

INSTALLATION

Symbol meaning
| Plug Weld
| Plug Weld

INSTALLATION POINT

1. After welding, apply undercoating to the corresponding parts. (See the paint / coating)
2. After applying the top coat, apply anti-rust agent to the internal panel portion of the closed section structural weld points.