# REAR SUSPENSION CROSSMEMBER > THREE-DIMENSIONAL DISTANCE

HINT:

1. In cases in which only one dimension is given, left and right are symmetrical.

1. For symbols, capital letters indicate right side of vehicle, small letters indicate left side of vehicle (seen from rear).

Measuring Point Name
Symbol | Name | Hole Diameter mm (in.)
A, a | Rear Suspension Member Installation Hole | φ55.2 (2.17)
B, b | Rear Suspension Lower Arm Installation Hole (Front) | 24.1X15.2 (0.95X0.60)
C, c | Stabilizer Installation Nut | M12 (0.47)
D, d | Rear Suspension Lower Arm Installation Hole (Rear) | φ7 (0.28)
E, e | Rear Suspension Member Installation Hole | φ67.6 (2.66)