# WORK NOTICES AND PRECAUTIONS > ANTI-RUST TREATMENT AFTER INSTALLATION OF BODY STRUCTURE PARTS OR OUTER PANELS

BODY SEALER APPLICATION

Text in Illustration
*1 | Sealer Gun

PURPOSE:

1. For water-proofing and anti-rust measures, always apply the body sealer to the body panel seams and hems of the doors, hood, etc.

NOTICE:

  Apply body sealer neatly to parts that require a high quality appearance.

UNDERCOAT APPLICATION

PURPOSE:

1. To prevent corrosion and protect the body from gravel, always apply a sufficient undercoating to the areas indicated.

VEHICLE BODY ANTI-RUST AGENT APPLICATION

PURPOSE:

1. The purpose is to protect areas from rust which are difficult to paint such as the backside of the box-shaped cross section frame parts.

METHOD:

1. Apply anti-rust agent through the service holes and/or installation holes of the parts.